#
SELECTOR INDICATOR LIGHT FUNCTION [FS5A-EL]

id051721103100
• The selector indicator light has a selector lever position light, and a gear position indicator light that indicates gear position.
• When downshifting is cancelled in the M range, the gear position indicator light flashes two times to alert the driver that downshifting is cancelled.
• If the ATF temperature reaches 130 °C {266 °F} or more while driving in manual shift mode, the gear position indicator illumination turns off and the transaxle switches to auto shift mode to reduce load on the ATX. After a period of time has passed and the ATF temperature decreases to 120 °C {248 °F} or less, the gear position indicator illumination turns back on and driving in manual shift mode is restored.