#
PRIMARY SHAFT COMPONENTS ASSEMBLY

D6E051517040103

1. Assemble in the order shown in the figure.

1 | Primary shaft
2 | Front bearing inner race (See Front Bearing Inner Race Assembly Note.)
3 | Snap ring
4 | 4th gear (See 4th Gear Assembly Note.)
5 | Spacer
6 | 3rd gear (See 3rd Gear Assembly Note.)
7 | 6th gear (See 6th Gear Assembly Note.)
8 | Rear bearing (See Rear Bearing Assembly Note.)
9 | Snap ring (See Rear Bearing Snap Ring Assembly Note.)

## Front Bearing Inner Race Assembly Note

1. Assemble the front bearing inner race using the SSTs and a press.

## 4th Gear Assembly Note

1. Install the 4th gear using the SST and a press.

## 3rd Gear Assembly Note

1. Install the 3rd gear using the SST and a press.

## 6th Gear Assembly Note

1. Install the 6th gear using the SST and a press.

## Rear Bearing Assembly Note

1. Install the rear bearing using the SST and a press.

## Rear Bearing Snap Ring Assembly Note

1. Install a new snap ring to the primary shaft.

2. Measure the clearance between the snap ring and the rear bearing inner race.

  • If not within the specification, adjust it by selecting a proper snap ring from below.

  Clearance between primary shaft rear bearing and snap ring
  0.0-0.1 mm {0.0000-0.0039 in}
  Snap ring size

  Identification mark | Thickness (mm {in}) | Identification mark | Thickness (mm {in})
  --- | --- | --- | ---
  A | 1.80 {0.071} | 3 | 2.20 {0.087}
  B | 1.85 {0.073} | 4 | 2.25 {0.089}
  C | 1.90 {0.075} | 5 | 2.30 {0.091}
  D | 1.95 {0.077} | 6 | 2.35 {0.093}
  E | 2.00 {0.079} | F | 2.40 {0.094}
  0 | 2.05 {0.081} | G | 2.45 {0.096}
  1 | 2.10 {0.083} | H | 2.50 {0.098}
  2 | 2.15 {0.085} | -