#
INSTRUMENT CLUSTER INSPECTION

id092200800400

## Speedometer

### Using the input/output check mode

1. Inspect the speedometer by setting it in the input/output check mode DTC 12.

### Using a speedometer tester

1. Adjust the tire air pressure to the specification.

2. Using a speedometer tester, verify that the speedometer indication is within the allowable ranges shown below.

Speedometer tester indication (km/h) | Allowable range (km/h)
--- | ---
20 | 20-24
40 | 40-44
60 | 60-64
80 | 80-85
100 | 100-105
120 | 120-126
140 | 140-146

Speedometer tester indication (mph) | Allowable range (mph)
--- | ---
10 | 10-12
20 | 20-22
30 | 30-32
40 | 40-43
50 | 50-53
60 | 60-63
70 | 70-73
80 | 80-84

3. Verify that fluctuation of the speedometer needle is within the allowable range.

  • If the speedometer needle does not move or the indication is outside of the allowable range, inspect the ABS (ABS/TCS) HU/CM (vehicles with ABS (ABS/TCS), DSC HU/CM (vehicles with DSC), PCM (vehicles without ABS) and related wiring harness.

  - If the ABS (ABS/TCS) HU/CM (vehicles with ABS (ABS/TCS), DSC HU/CM (vehicles with DSC), PCM (vehicles without ABS) and related wiring harness are normal, replace the instrument cluster.

  Needle fluctuation allowable range
  Within 3.0 km/h

## Tachometer

### Using the input/output check mode

1. Inspect the tachometer by setting it in the input/output check mode DTC 13.

### Using the SSTs (WDS or equivalent)

  Caution

  • If the engine speed exceeds the allowable range, the engine could be damaged. Therefore, when inspecting the tachometer, do not allow the engine speed to exceed the allowable range indication on the tachometer.

1. Connect the SSTs (WDS or equivalent) to the vehicle DLC-2 16-pin connector.

2. Access and monitor PIDs by SSTs (WDS or equivalent).

## Fuel Gauge

1. Inspect the fuel gauge by setting it in the input/output check mode DTC 23.

## Water Temperature Gauge

1. Inspect the water temperature gauge by setting it in the input/output check mode DTC 25.