#
RELAY INSPECTION

id092100800300

## Relay Type

Terminal type | Parts name
--- | ---
Four-terminal | Type A | • Main relay • Fuel pump relay • Starter relay • TNS relay • Front fog light relay • Rear fog light relay • Horn relay • Rear window defroster relay • Woofer relay • A/C relay • Blower relay • Cooling fan relay No.1 (except L3 engine) • Cooling fan relay No.2 • Cooling fan relay No.3 • Cooling fan relay No.4 • ETC relay
Type B | • Headlight relay • Glow relay (MZR-CD (RF Turbo) engine only)
Five-terminal | Type C | • Cooling fan relay No.1 (L3 engine only)

## Four-terminal

### Type A

1. Remove the relay.

2. Inspect for continuity between the relay terminals using a tester.

  • If there is any malfunction, replace the relay.

### Type B

1. Remove the relay.

2. Inspect for continuity between the relay terminals using a tester.

  • If there is any malfunction, replace the relay.

### Type C

1. Remove the relay.

2. Inspect for continuity between the relay terminals using a tester.

  • If there is any malfunction, replace the relay.