#
DTC P0403 [L8, LF, L3]

id0102a1807100

DTC P0403 | EGR valve (stepper motor) circuit problem
--- | ---
DETECTION CONDITION | • The PCM monitors the input voltage from EGR valve. If the voltage remain low or high, the PCM determines that the EGR valve circuit has a malfunction. Diagnostic support note • This is a continuous monitor (CCM). • The MIL illuminates if the PCM detects the above malfunction conditions in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM. • PENDING CODE is available if the PCM detects the above malfunction condition during first drive cycle. • FREEZE FRAME DATA is available. • Are any DTCs is stored in the PCM memory.
POSSIBLE CAUSE | • EGR valve malfunction • Connector or terminal malfunction • Short to power supply in wiring harness between EGR valve terminal E and PCM terminal 2K • Short to power supply in wiring harness between EGR valve terminal A and PCM terminal 2G • Short to power supply in wiring harness between EGR valve terminal B and PCM terminal 2L • Short to power supply in wiring harness between EGR valve terminal F and PCM terminal 2H • Short to ground circuit in wiring harness between EGR valve terminal E and PCM terminal 2K • Short to ground circuit in wiring harness between EGR valve terminal A and PCM terminal 2G • Short to ground circuit in wiring harness between EGR valve terminal B and PCM terminal 2L • Short to ground circuit in wiring harness between EGR valve terminal F and PCM terminal 2H • Open circuit in wiring harness between EGR valve terminal E and PCM terminal 2K • Open circuit in wiring harness between EGR valve terminal A and PCM terminal 2G • Open circuit in wiring harness between EGR valve terminal B and PCM terminal 2L • Open circuit in wiring harness between EGR valve terminal F and PCM terminal 2H • Open circuit in wiring harness between main relay terminal D and EGR valve terminal C • Open circuit in wiring harness between main relay terminal D and EGR valve terminal D • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA AND DIAGNOSTIC MONITORING TEST RESULTS HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service information. If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT EGR VALVE FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect EGR valve connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminals and/or connector, then go to Step 10.
No | Go to the next step.
4 | INSPECT POWER CIRCUIT FOR OPEN CIRCUIT • Turn the ignition switch to the ON position (Engine off). • Measure the voltage following terminal and body ground. - EGR valve terminal C - EGR valve terminal D • Is the voltage B+? | Yes | Go to the next step.
No | Repair or replace the wiring harness for an open circuit then go to Step 10.
5 | INSPECT EGR VALVE • Inspect the EGR valve. (See EGR VALVE INSPECTION [L8, LF, L3].) • Is the EGR valve normal? | Yes | Go to the next step.
No | Replace the EGR valve, then go to Step 10.
6 | INSPECT FOR CONTROL CIRCUIT FOR SHORT TO GROUND • Turn the ignition switch off. • Inspect for continuity between the following terminal and body ground: - EGR valve terminal E - EGR valve terminal A - EGR valve terminal B - EGR valve terminal F • is there continuity? | Yes | Repair or replace the wiring harness for short to ground, then go to Step 10.
No | Go to the next step.
7 | INSPECT FOR CONTROL CIRCUIT FOR SHORT TO POWER • Turn the ignition switch to the ON position (Engine off). • Measure the voltage following terminal and body ground: - EGR valve terminal E - EGR valve terminal A - EGR valve terminal B - EGR valve terminal F • Is the voltage B+? | Yes | Repair or replace the wiring harness for short to power supply, then go to Step 10.
No | Go to the next step.
8 | INSPECT PCM FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminals and/or connector, then go to Step 10.
No | Go to the next step.
9 | INSPECT CONTROL CIRCUIT FOR OPEN CIRCUIT • Remove the PCM with the PCM connector connected. • Inspect for continuity following terminals: - Between EGR valve terminal E and PCM terminal 2K - Between EGR valve terminal A and PCM terminal 2G - Between EGR valve terminal B and PCM terminal 2L - Between EGR valve terminal F and PCM terminal 2H • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for an open circuit then go to the next step.
10 | VERIFY TROUBLESHOOTING OF DTC P0403 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the PENDING CODE for this DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [L8, LF, L3].)
No | Go to the next step.
11 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [L8, LF, L3].) • Are any DTC present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [L8, LF, L3].)
No | Troubleshooting completed.