#
CRUISE CONTROL OPERATION [MZR-CD (RF Turbo)]

id0140f1184300

## Operating Conditions

• The PCM can execute cruise control when the following conditions are met:

  - Cruise control main switch is ON.
  - Brake pedal is released.
  - Clutch pedal is released.
  - Gear is not neutral position.
  - Vehicle speed of 27 km/h {16.7 mph} or more.
  - No DTC is stored. (However, even if the PCM detects a cruise control system malfunction (in brake switch or cruise control switch), if the cruise control system is normal after the engine switch is turned to the ON position, the cruise control system is operable.)

## Driving At Set Speed

• Once the desired speed has been set, the PCM determines the fuel injection amount based on the vehicle speed signal.
• If the actual vehicle speed goes below the set speed, the PCM increases the fuel injection amount, and if it goes above the set speed the PCM decreases the fuel injection amount.

## Tap Up/Tap Down Operation

• When driving at a set speed, if the SET/COAST or RESUME/ACCEL signal is input to the PCM for a very short interval, the set speed will be increased or decreased respectively by 1.6 km/h {1.0 mph}.

## Cancel Condition of Cruise Control System

• When the vehicle speed becomes less than 22.5 km/h {14.0 mph}, the cruise control system operation is canceled, however the speed set in the memory is not cleared.
• The cruise control system operation is cancelled if any signal from the clutch switch, neutral switch, or cruise control cancel switch, or brake signal is input.