#
CONNECTING ROD SIDE CLEARANCE INSPECTION [WITH DIESEL PARTICULATE FILTER]

id0110f3503000

1. Install the connecting rod cap. (See Connecting Rod Cap Assembly Note)

2. Measure the connecting rod large end side clearance. Replace the connecting rod and cap if necessary.

Standard clearance

  0.110-0.262 mm {0.0044-0.0103 in}

Maximum clearance

  0.512 mm {0.0202 in}

3. Remove the connecting rod cap.