#
COOLING FAN MOTOR INSPECTION [MZR-CD (RF Turbo)]

id0112f1801800

1. Verify that the battery is fully charged. (See BATTERY INSPECTION [MZR-CD (RF Turbo)].)

2. Disconnect the cooling fan motor connector.

3. Install a tester and battery to the cooling fan motor connector as shown in the figure.

4. Verify that fan motor operates smoothly at the standard current.

  • If not within the specification, replace the fan motor.

Cooling fan motor current

  No.1: 4.4-7.4 A
  No.2: 6.5-9.5 A