#
DTC P2227 [MZR-CD (RF Turbo)]

id0102f1840700

DTC P2227 | BARO sensor range/performance malfunction
--- | ---
DETECTION CONDITION | • The PCM monitors the input signal from the barometric pressure sensor. If the difference between the barometric pressure input from the barometric pressure sensor and the manifold absolute pressure is more than 10 kPa {75 mmHg, 3.0 inHg}, the PCM determines that there is a malfunction in the barometric pressure sensor. Diagnostic support note • The MIL illuminates if the PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM. • PENDING CODE is available if the PCM detects the above malfunction condition during the first drive cycle. • FREEZE FRAME DATA is available. • DTC is stored in the PCM memory.
POSSIBLE CAUSE | • BARO sensor (integrated in PCM) malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY CURRENT SIGNAL STATUS: IS CONCERN INTERMITTENT OR CONSTANT? • Connect the WDS or equivalent to the DLC-2. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the PENDING CODE for this DTC present? | Yes | Go to the next step.
No | Intermittent concern exists. Perform the "INTERMITTENT CONCERN TROUBLESHOOTING". (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
4 | VERIFY TROUBLESHOOTING OF DTC P2227 COMPLETED • Make sure to reconnect all disconnected connectors. • Turn the engine switch to the ON position (Engine off). • Clear the DTC from the memory using the WDS or equivalent. • Perform the Repair Verification Drive Mode. (See OBD DRIVE MODE [MZR-CD (RF Turbo)].) • Is the PENDING CODE for this DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | No concern is detected. Go to the next step.
6 | VERIFY AFTER REPAIR PROCEDURE • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | Troubleshooting completed.