#
CARD KEY BATTERY REPLACEMENT [WITH ADVANCED KEYLESS SYSTEM]

id0914z68061b2

## Card Key Type

1. Pull out the auxiliary key.

2. Replace the cap using a flathead screwdriver, then rotate and remove the cap.

  Caution

  • Do not turn the cap excessively. The cap may be damaged.

3. Insert a flathead screwdriver into the crack and press the battery out.

4. Insert the new battery (CR2025) with the positive pole (+) facing the (+) mark on the cap.

Battery specification

  Lithium CR2025 × 1

  Note

  • The batteries will last about 1 years when used 10 times a day.

5. Rotate and close the cap.

6. Reinsert the auxiliary key.