#
PANEL LIGHT CONTROL SWITCH REMOVAL/INSTALLATION

id091800806500

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Panel light control switch (See Panel Light Control Switch Removal Note.)
2 | Connector

3. Install in the reverse order of removal.

## Panel Light Control Switch Removal Note

1. Insert your hand from the lower side of the dashboard and squeeze the tabs of the panel light control switch.

2. Pull the panel light control switch outward to remove it.