#
NOISE FILTER REMOVAL/INSTALLATION [WGN]

id0920008064b4

## Brake Light Noise Filter

1. Remove the noise filter according to the NOISE FILTER REMOVAL/INSTALLATION procedure for the 4SD.

2. Install in the reverse order of removal.

## Rear Window Defroster Noise Filter

1. Disconnect the negative battery cable.

2. Remove the liftgate lower trim.

3. Remove in the order indicated in the table.

1 | Bolt
2 | Screw
3 | Connector
4 | Noise filter

4. Install in the reverse order of removal.