#
WHEEL ALIGNMENT PRE-INSPECTION

id021100119800

1. Inspect the tire inflation, and adjust to the recommended pressure as necessary.

2. Inspect the front wheel bearing play and correct it if necessary. (See Wheel Bearing Play Inspection.)

3. Inspect the wheel and tire runouts. (See SUSPENSION TECHNICAL DATA.)

4. Inspect the ball joints and steering linkage for excessive looseness.

5. Shake the vehicle to inspect the operation of the shock absorbers.

  Note

  • The vehicle must be on level ground and unloaded.
  • Unloaded: Fuel tank is full. Engine coolant and engine oil are at specified level. Spare tire, jack and tools are in designated position.

6. Measure the height from the center of the wheel to the fender brim. The difference between the left and right measurement must not exceed 10 mm {0.39 in}.