#
FRONT FOG LIGHT BULB REMOVAL/INSTALLATION

id091800468600

## Type A

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Cover
2 | Connector
3 | Front fog light bulb (See Front fog light bulb removal note.)

  Caution

  • A halogen bulb generates extremely high heat when it is used. If the surface of the bulb is soiled, excessive heat will build up and the light's life will be shortened. When replacing the bulb, hold the metal flange, not the glass.

3. Install in the reverse order of removal.

### Front fog light bulb removal note

1. Release the bulb pressing wire to remove the front fog light bulb.

## Type B

1. Disconnect the negative battery cable.

2. Slightly bend back the mudguard.

3. Disconnect the front fog light bulb connector and remove the front fog light bulb by turning it in the direction of the arrow.

  Caution

  • A halogen bulb generates extremely high heat when it is used. If the surface of the bulb is soiled, excessive heat will build up and the light's life will be shortened. When replacing the bulb, hold the metal flange, not the glass.

4. Install in the reverse order of removal.