#
REFRIGERANT PRESSURE SWITCH REMOVAL/INSTALLATION

id074000802600

1. Remove the battery.

2. Discharge the refrigerant from the system. (See REFRIGERANT RECOVERY.) (See REFRIGERANT CHARGING.)

3. Loosen the refrigerant pressure switch using two spanners.

4. Remove in the order indicated in the table.

1 | Refrigerant pressure switch connector
2 | Refrigerant pressure switch (See Refrigerant Pressure Switch Installation Note.)

5. Install in the reverse order of removal.

## Refrigerant Pressure Switch Installation Note

1. Apply compressor oil to O-ring and connect the joint.