#
PID/DATA MONITOR TABLE [ADVANCED KEYLESS SYSTEM]

id0902e2862100

PID/data monitor table

PID name (definition) | Data contents | Unit/Operation | Terminal
--- | --- | --- | ---
DTC_CNT | Number of continuous DTCs | - | -
RPM | Engine speed | RPM | 3Z, 3AA
VSS | Vehicle speed | KPH | 3Z, 3AA
VPWR | Supply voltage | V | 2D
NUMCARD | Number of programmed card keys | - | -
NUMKEY* | Number of programmed key ID numbers | - | -
DRSW_D | Door switch (Driver's door) | OPEN/CLOSE | 2R
DRSW_ALL | Door switch (All doors and liftgate) | OPEN/CLOSE | 2R
REQ_SW_D | Request switch (Driver's door) | On/Off | 3H
REQ_SW_P | Request switch (Passenger door) | On/Off | 3J
REQ_SW_BK | Request switch (Trunk lid/Liftgate) | On/Off | 3L
LOCK_SW_D | Door lock-link switch | On/Off | 3E
IMMOBI | Immobilizer system equipped or not | On*/Off | -
TR/LG_SW | Trunk/liftgate latch switch | OPEN/CLOSE | 2R
IG_KEY_IN | Key reminder switch | Key-In/Key-Out | 2O
IG_SW_ST | Ignition switch (Push switch) | Pushed/Not Pushed | 2N
BUZZER | Keyless buzzer | On/Off | 3Y
PWR_IG1 | Power supply (IG1) | On/Off | 2B
PWR_ACC | Power supply (ACC) | On/Off | 2I

  * :
Vehicles with immobilizer system

ACTIVE COMMAND MODE TABLE [ADVANCED KEYLESS SYSTEM]

Command name | Output part name | Unit/Operation | Terminal
--- | --- | --- | ---
BZR_OUT | Keyless buzzer | On/Off | 3Y
BZR_INN | Interior buzzer (Instrument cluster) | On/Off | 3Z, 3AA
LNP_RED | Keyless warning light (red) | On/Off | 3Z, 3AA
LNP_GREEN | Keyless indicator light (green) | On/Off | 3Z, 3AA
HAZARD | Hazard flashers | On/Off | 2R
DR_LOCK | All doors Lock/Off | Lock/Off | 2R
DR_UNLOCK | All doors Unlock/Off | Unlock/Off | 2R
SUPELROCK | All doors Lock/Off | Lock/Off | 2R