#
DRIVELINE/AXLE TECHNICAL DATA

id035000800100

Item | Specification
--- | ---
Maximum front wheel bearing play | 0.05 mm {0.002 in}
Maximum rear wheel bearing play | 0.05 mm {0.002 in}
Front drive shaft standard length (ATX) | LH: 674.6-684.6 mm {26.56-26.95 in} RH: 631.0-641.0 mm {24.85-25.23 in}
Front drive shaft standard length (MTX) | L8, LF (LH): 677.7-687.7 mm {26.69-27.07 in} L8, LF (RH) and L3 (2WD/RH): 627.9-637.9 mm {24.73-25.11 in} L3 (2WD/LH): 676.5-686.5 mm {26.64-27.02 in} L3 Turbo and MZR-CD (RF Turbo) (LH): 640.4-650.4 mm {25.22-25.60 in} L3 Turbo and MZR-CD (RF Turbo) (RH): 584.1-594.1 mm {23.00-23.38 in}
Rear drive shaft standard length | LH: 804.2-814.2 mm {31.67-32.05 in} RH: 860.7-870.7 mm {33.89-34.27 in}
Differential oil | Grade: API service GL-5 Viscosity: SAE 80W-90 Capacity (Approximate quantity): 1.00 L {1.06 US qt, 0.88 Imp qt}
Rear differential oil type | Grade: API service GL-5 Viscosity: SAE 80W-90
Rear differential oil capacity (approximate quantity) | 1.00 L {1.06 US qt, 0.88 Imp qt}
Rear differential pinion height | -0.032-0.032 mm {-0.0012-0.0012 in}
Rear differential drive pinion preload | 1.3-1.8 N·m {13.3-18.2 kgf·cm, 11.5-15.9 in·lbf}
Rear differential backlash of drive pinion and ring gear | Standard: 0.09-0.11 mm {0.003-0.004 in} Minimum value: 0.05 mm {0.002 in}
Maximum propeller shaft runout [A26MX-R] | 0.3 mm {0.012 in}
Propeller shaft starting torque [A26MX-R] | Rear Differential side: 0.29-0.98 N·m {3.0-9.9 kgf·cm, 2.6-8.6 in·lbf} Others: 0.29-1.18 N·m {3.0-12.0 kgf·cm, 2.6-10.4 in·lbf}
Propeller shaft runout limit [JA5AX-EL] | 0.3 mm {0.01 in}
Propeller shaft starting torque [JA5AX-EL] | 0.29-0.78 N·m {3.0-7.9 kgf·cm, 2.7-6.8 in·lbf}
Transfer oil [A26MX-R] | Specified oil grade: API Service GL-5 Specified oil viscosity: SAE 80W-90 Capacity (approximate quantity): 1.2 L {1.3 US qt, 1.1 lmp qt}
Transfer oil [JA5AX-EL] | Specified oil grade: API Service GL-5 Specified oil viscosity: SAE 80W-90 Capacity (approximate quantity): 0.62 L {0.65 US qt, 0.54 lmp qt}