#
APRON REINFORCEMENT COMPONENT INSTALLATION

D6E098053260B02

1. When installing new parts, measure and adjust the body as necessary to conform with standard dimensions.

2. Drill holes for plug welds before installing new parts.

3. Install in the following order: apron reinforcement (lower), apron reinforcement (rear), and apron reinforcement (upper).

  Note

  • After installing, fillet weld in location (A).

  Caution

  • When fillet welding, be careful of dripping, melted.

4. After temporarily installing new parts, make sure the related parts fit properly.