#
STARTER INTERLOCK SWITCH CONSTRUCTON/OPERATION [General (L.H.D.) specs. (MTX)]

id0119a31310a9

## Construction

• The starter interlock switch mechanism prevents vehicle surge when the engine is started, enhancing the safety. The engine cannot be started unless the clutch is depressed.
• The mechanism is provided with a starter interlock switch on the circuit between the ignition switch and the starter.

1 | Starter interlock switch
2 | Clutch pedal
3 | Pedal bracket
4 | Rod

## Operation

• Depressing the clutch pedal presses the starter interlock switch rod. At this time, the starter interlock switch is on, and the power circuit to starter closes. Accordingly, the starter operates only when the clutch is depressed whereby the engine can be started.

1 | Starter interlock switch internal circuit
2 | Clutch pedal depressed: ON
3 | Top view
4 | Side view
5 | Operating direction
6 | ON
7 | OFF
8 | Starter interlock switch
9 | Rod