#
RECLINER MOTOR INSPECTION

id091300801000

1. Disconnect the recliner motor connector.

2. Inspect the recliner motor operation when B+ is applied to the terminal as shown.

  • If not as specified, replace the seat cushion frame.

Motor operation | Connection
--- | ---
B+ | GND
Forward | A | D
Backward | D | A

3. Connect battery positive voltage to front tilt motor terminal B and connect terminal C to ground.

4. Operate the front tilt motor and measure the voltage at terminals B and C.

  • If there is any malfunction, replace the recliner motor.