#
NO. 2 DOOR GLASS DOES NOT OPERATE USING THE KEYLESS TRANSMITTER

id090397821500

2 | DOOR GLASS DOES NOT OPERATE USING THE KEYLESS TRANSMITTER
POSSIBLE CAUSE | • Keyless control module malfunction • BCM malfunction • Open circuit in wiring harness between keyless control module and BCM • Any door or trunk lid/liftgate is open • Key is inserted in steering lock

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | • Inspect the door lock/unlock operation using the transmitter. • Does it operate normally? | Yes | Inspect the following parts, and repair or replace. • BCM (See BODY CONTROL MODULE (BCM) INSPECTION.) • Keyless control module (Vehicles with advanced keyless system) (See KEYLESS CONTROL MODULE INSPECTION [WITH ADVANCED KEYLESS SYSTEM].)
No | Go to the next step.
2 | • Inspect the open/close condition of the doors and the trunk lid/liftgate. • Is the reason why they do not lock/unlock because a door or the trunk lid/liftgate is open? | Yes | System is normal (Does not operate when a door or the trunk lid/liftgate is open).
No | Go to the next step.
3 | • Verify whether the key is in the steering lock. • Is the reason why they do not lock/unlock because the key is inserted in the steering lock? | Yes | System is normal (Does not operate when the key is inserted in the steering wheel lock)
No | Go to the next step.
4 | • When the lock/unlock operation does not operate for reasons other than the above Steps 2 and 3. | Yes | Inspect the following parts, and repair or replace. • Keyless control module (See KEYLESS CONTROL MODULE INSPECTION [WITH ADVANCED KEYLESS SYSTEM].) • Wiring harness between keyless control module and BCM.
No | Reinspect for malfunction recurrence.If the malfunction is not corrected, repeat the procedure from Step 1.