#
COOLING FAN COMPONENT CONSTRUCTION [L8, LF, L3]

id0112b21005b1
• The cooling fan component consists of the radiator cowling, cooling fans, and cooling fan motors.
• Electric cooling fans No.1 and No.2, which operate according to the fan control signal from the PCM, have been adopted. Due to this, engine noise has been reduced and rapid engine warming-up is possible.
• The radiator cowling and cooling fans are made of plastic for weight reduction.
• Coolant reserve tank can be removed from the radiator cowling.

.

1 | Type A
2 | Type B
3 | Type C
4 | Cooling fan component
5 | Cooling fan No.1
6 | Cooling fan No.2
7 | Radiator cowling
8 | Coolant reserve tank
9 | Cooling fan motor No.1
10 | Cooling fan motor No.2

Cooling fan, cooling fan motor specification

Item | Specification
--- | ---
Type A | Type B | Type C
Cooling fan No.1 (LH) | Number of blades |  | 5 | 7 | 7
Motor output | (W) | 80 | 120 | 70
Outer diameter of fan | (mm {in}) | 320 {12.6}
Cooling fan No.2 (RH) | Number of blades |  | 7 | 5 | 4
Motor output | (W) | 80 | 120 | 90
Outer diameter of fan | (mm {in}) | 320 {12.6}