#
CAMSHAFT INSPECTION [WITH DIESEL PARTICULATE FILTER]

id0110f3501500

1. Set No.1 and No.6 journals on V-blocks. Measure the camshaft runout. Replace the camshaft if necessary.

Maximum runout

  0.03 mm {0.0012 in}

2. Measure the cam lobe height at the two points as shown. Replace the camshaft if necessary.

Standard height

  IN: 40.140 mm {1.5803 in}
  EX: 39.809 mm {1.5673 in}

Minimum height

  IN: 39.940 mm {1.5724 in}
  EX: 39.609 mm {1.5594 in}

3. Measure the journal diameters in X and Y directions at the two points (A and B) as shown. Replace the camshaft if necessary.

Standard diameter

  31.950-31.975 mm {1.2579-1.2588 in}

Minimum diameter

  31.920 mm {1.2567 in}