#
INTERMEDIATE SENSOR INSPECTION [JA5AX-EL]

id051705807100

## On-Vehicle Inspection

1. Disconnect the terminal component No.2 connector.

2. Measure resistance between the terminals C and D.

  • If not as specified, inspect the intermediate sensor. (See Inspection of Individual Part.)

Intermediate sensor

  Resistance: 513-627 ohms (ATF temperature: 20 °C {68 °F})

3. Connect the terminal component No.2 connector.

## Inspection of Individual Part

1. Remove the intermediate sensor. (See INTERMEDIATE SENSOR REMOVAL/INSTALLATION [JA5AX-EL].)

2. Measure resistance between the terminals of the intermediate speed sensor.

  • If not as specified, replace the intermediate sensor.
  • If it is normal, replace the harness.

Intermediate sensor

  Resistance: 513-627 ohms (ATF temperature: 20 °C {68 °F})

3. Install the intermediate sensor. (See INTERMEDIATE SENSOR REMOVAL/INSTALLATION [JA5AX-EL].)