#
PID/DATA MONITOR TABLE [BCM]

id0902j0862100

PID/data monitor item | Input/output part | Unit/Condition (Tester display) | BCM terminal
--- | --- | --- | ---
CCNT_GE | DTC | - | -
HOOD_SW | bonnet switch | OPEN/CLOSE | 8M
TR/LG_SW | Trunk compartment light switch | OPEN/CLOSE | 2F
DRSW_REAR | Rear door switch (LH/RH) | OPEN/CLOSE | 7D, 1F
DRSW_P | Front door switch (passenger's side) | OPEN/CLOSE | 7F
DRSW_D | Front door switch (driver's side) | OPEN/CLOSE | 7B
HAZARD | Hazard warning switch | On/Off | 4G
WPINT_REAR | Rear wiper switch (INT position) | On/Off | 4I
TURN_SW_R | Turn switch (RH) | On/Off | 4E
TURN_SW_L | Turn switch (LH) | On/Off | 4C
LLSW_D | Driver-side door lock-link switch | LOCK/UNLOCK | 7C, 7E
LLSW_P_R | Except driver-side door lock-link switch | LOCK/UNLOCK | 7G