#
ELECTRONIC THROTTLE CONTROL OUTLINE [L8, LF, L3]

id0140a5100700
• By controlling the throttle actuator, the PCM sets an optimal throttle valve opening angle according to the engine conditions.
• The PCM calculates a target throttle valve opening angle based on the accelerator pedal depression amount. The PCM sends electrical current to the throttle actuator to achieve the target opening angle.
• The engine idling speed can be controlled through PCM control of the throttle valve. Due to this, the previous IAC valve has been eliminated.