#
NO.10 FREQUENT SHIFTING [JA5AX-EL]

id050305801500

10 | Frequent shifting
DESCRIPTION | • Downshifting occurs immediately even when accelerator pedal depressed slightly in D range.
POSSIBLE CAUSE | • The circuit which is the cause is basically the same as for No.9 "Abnormal shifting". However, a malfunction of input signal to TP sensor, input/turbine speed sensor, VSS (including the sensor ground, sensor harness and connector), or clutch slippage (clutch stuck, low pressure in line) may also be the cause. Note • Before following troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.