#
BASE UNIT OUTLINE

id092000107600
• The base unit controls the AM/FM tuner, lower modules.
• An auto level control (ALC) function that controls speaker volume according to vehicle speed has been adopted.
• For drive information system (DIS) equipped vehicles, a CAN communication control circuit is included in the base unit. The base unit receives, using the CAN system, the DIS display signal from the instrument cluster, and converts it to a signal sent to the information display (See DRIVE INFORMATION SYSTEM OUTLINE.) (See DRIVE INFORMATION SYSTEM STRUCTURAL VIEW.) (See DRIVE INFORMATION SYSTEM WIRING DIAGRAM.) (See DRIVE INFORMATION SYSTEM OPERATION.) (See DRIVE INFORMATION SYSTEM CONSTRUCTION.)