#
NO. 3 DOOR GLASS DOES NOT OPERATE USING THE REQUEST SWITCH

id090397821700

3 | Door glass does not operate using the request switch
POSSIBLE CAUSE | • Keyless control module malfunction • BCM malfunction • Open circuit in wiring harness between request switch and keyless control module. • Any door or trunk lid/liftgate is open. • Key is inserted in steering lock. • Start knob is in a position other than LOCK position.

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | • Verify the door lock/unlock operation by operating the request switch. • Does it operate normally? | Yes | Inspect the following parts, and repair or replace. • Keyless control module (See KEYLESS CONTROL MODULE INSPECTION [WITH ADVANCED KEYLESS SYSTEM].) • BCM (See BODY CONTROL MODULE (BCM) INSPECTION.)
No | Go to the next step.
2 | • Verify the open/close condition of the doors and the trunk lid/liftgate. • Is the reason why they do not lock/unlock because a door or the trunk lid/liftgate is open? | Yes | The system is normal (When any door or the trunk lid/liftgate is open, the system does not operate).
No | Go to the next step.
3 | • Verify the start knob position, or if the key is in the steering lock. • Is the reason why the door lock/unlock does not operate because the start knob is in a position other than LOCK, or the key is inserted? | Yes | The system is normal (When the start knob is in a position other than LOCK, or the key is inserted in the steering lock, the system does not operate).
No | Go to the next step.
4 | • The door lock/unlock does not operate for reasons other than Steps 2 and 3 above. | Yes | Inspect the following parts, and repair or replace. • Keyless control module (See KEYLESS CONTROL MODULE INSPECTION [WITH ADVANCED KEYLESS SYSTEM].) • Wiring harness between the request switch and the keyless control module.
No | Reinspect for malfunction recurrence.If the malfunction is not corrected, repeat the procedure from Step 1.