#
PCM CONFIGURATION [MZR-CD (RF Turbo)]

id0140f1802600

1. Connect the WDS or equivalent to DLC-2.

2. Set up the WDS or equivalent (including the vehicle recognition).

3. Select "Module programming."

4. Select "Programmable Module Installation."

5. Select "PCM" and perform procedures according to directions on the WDS or equivalent screen.

  Note

  • If the PCM is replaced with a new one, the PCM stores DTCs P0602 and P1675, illuminates the MIL even though no malfunction is detected. When the configuration is completed, DTCs P0602 and P1675 are cleared.

6. Retrieve DTC's using the WDS or equivalent, then verify that DTCs are present.

  • If a DTC is present, perform the applicable DTC inspection.