#
COOLING FAN MOTOR INSPECTION [L3 Turbo]

id0112b28018b3

  Note

  • Cooling fan motor No.2 can be inspected, however, cooling fan motor No.1 cannot be inspected because it is integrated with the fan control module.

1. Verify that the battery is fully charged. (See BATTERY INSPECTION [L8, LF, L3, L3 Turbo].)

2. Disconnect the cooling fan motor No.2 connector (2 terminals).

3. Install a tester and battery to the cooling fan motor No.2 connector (2 terminals) as shown in the figure.

4. Verify that fan motor No.2 operates smoothly at the standard current.

  • If not within the specification, replace the fan motor No.2.

Cooling fan motor No.2 current

  12.8-16.8 A