#
CLUTCH PEDAL POSITION (CPP) SWITCH CONSTRUCTION/OPERATION [L8, LF, L3 MTX]

id0140a51777a8
• When the clutch pedal is depressed, the contact closes (ON) and the PCM detects a voltage of 0 V. When the clutch pedal is not depressed, the contact opens (OFF) the PCM detects a voltage of 12 V.

1 | CPP switch
2 | Push OFF
3 | Clutch pedal not depressed (OFF)
4 | Clutch pedal depressed (ON)
5 | Clutch pedal depressed (ON)
6 | Clutch pedal not depressed (OFF)
7 | No load
8 | Load