#
MEMORY CLEARING PROCEDURE

id0902f6803900

1. Start the on-board diagnostic test mode.

2. While pressing the POWER button, simultaneously press the AUDIO CONT button for 2 s or more.

1 | POWER button (with RDS)
AUDIO CONT button (without RDS)
2 | AUDIO CONT button (with RDS)
POWER button (without RDS)

  Caution

  • Before clearing the memory, be sure to enter all of the DTCs displayed in the on-board diagnostic test mode in the Audio Repair Order Form.

3. To stop the on-board diagnostic test mode, turn the ignition switch off.