#
FUEL PUMP RESISTOR REMOVAL/INSTALLATION [L3 Turbo]

id0114b4801200

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF, L3, L3 Turbo].)

2. Remove the air cleaner. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

3. Disconnect the fuel pump resistor connector.

4. Remove in the fuel pump resistor.

5. Install in the order as shown in the figure.

Tightening torque

  4.2-6.2 N·m {43-63 kgf·cm, 38-54 in·lbf}

6. Connect the fuel pump resistor connector.