#
ONE-WAY CLUTCH OUTLINE

D6E051719500A17

## One-Way Clutch No.1

• The one-way clutch No.1 locks the counterclockwise rotation (seen from the torque converter side) of the front internal gear. The one-way clutch No.1 operates in D, and M range of the 1GR.

## One-Way Clutch No.2

• The one-way clutch No.2 locks the clockwise rotation (seen from the torque converter side) of the direct clutch drum. The one-way clutch No.2 operates in D, and M range of the 1GR, 2GR, 3GR and 4GR.