#
NO. 3 ALL POWER WINDOWS OTHER THAN DRIVER'S SIDE DO NOT OPERATE USING THE POWER WINDOW SUBSWITCH

id0903j5831200

3 | All power windows other than driver's side do not operate using the power window subswitch.
POSSIBLE CAUSE | • Open or short circuit in power window subswitch wiring harness (battery power supply circuit). • Power window subswitch malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Turn the ignition switch to the ON position. • Set the power cut-switch to the UNLOCK position. • Measure the voltage at the power window subswitch terminal D. • Is the voltage B+? | Yes | Replace the power window subswitch. (See POWER WINDOW SWITCH REMOVAL/INSTALLATION.)
No | Inspect for an open or short circuit in the wiring harness between the power window main switch and the power window subswitch. Inspect the power window subswitch connector connection. (damage/pulled-out pins, corrosion) Repair or replace if necessary.