#
PURGE SOLENOID VALVE INSPECTION [L8, LF, L3]

id0116a4800900

## Airflow Inspection

  Note

  • Perform the following test only when directed.

1. Disconnect the negative battery cable.

2. Remove the purge solenoid valve. (See PURGE SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF, L3].)

3. Inspect airflow between the ports under the following conditions.

  • If not as specified, replace the purge solenoid valve.
  • If as specified, carry out the "Circuit Open/Short Inspection".

## Circuit Open/Short Inspection

1. Disconnect the PCM connector. (See PCM REMOVAL/INSTALLATION [L8, LF, L3].)

2. Inspect the following wiring harness for open or short (continuity check).

Open circuit

  • If there is no continuity, the circuit is open. Repair or replace the harness.

  - Purge solenoid valve terminal A (harness-side) and PCM terminal 4U
  - Purge solenoid valve terminal B (harness-side) and main relay terminal C (harness-side)

Short circuit

  • If there is continuity, the circuit is shorted. Repair or replace the harness.

  - Purge solenoid valve terminal A (harness-side) and body GND
  - Purge solenoid valve terminal B (harness-side) and power supply