#
HVAC FEATURES

id070000100200

Improved air conditioning performance | • A sub-cooling system integrating the condenser and receiver/drier has been adopted to facilitate evaporator operation. This system also reduces the number of parts and the amount of refrigerant.
Improved visibility | • To improve windshield and front door glass defogging, the climate control unit is designed to automatically turn the air intake mode to FRESH when the airflow mode selector dial is turned to DEFROSTER position. (manual air conditioner)
Reduce Weight | • The A/C unit integrating the cooling unit and heater unit has been adopted to reduce weight.
Improved comfort | • Water heater system adopted (For MZR-CD (RF Turbo) European (L.H.D.) specs.)