#
REAR DRAIN HOSE REMOVAL [WGN]

id0915008015a4

1. Disconnect the negative battery cable.

2. Turn the seaming welt and weatherstrip over.

3. Remove the sunroof seaming welt.

4. Remove the A-pillar trims.(See A-PILLAR TRIM REMOVAL.)

5. Remove the B-pillar upper trims.(See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

6. Remove the C-pillar trims.(See C-PILLAR TRIM REMOVAL/INSTALLATION [WGN].)

7. Remove the D-pillar trims.(See D-PILLAR TRIM REMOVAL/INSTALLATION [WGN].)

8. Remove the front map light.(See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

9. Remove the rear map light.(See REAR MAP LIGHT REMOVAL/INSTALLATION.)

10. Remove the cargo compartment light.(See CARGO COMPARTMENT LIGHT REMOVAL/INSTALLATION [WGN].)

11. Remove the sunvisors.(See (SUNVISOR REMOVAL/INSTALLATION.)

12. Remove the assist handle.(See ASSIST HANDLE REMOVAL/INSTALLATION.)

13. Remove the net anchor.

14. Remove the headliner.(See HEADLINER REMOVAL/INSTALLATION [WGN].)

15. Remove the trunk side trim.(See TRUNK SIDE TRIM REMOVAL/INSTALLATION [WGN].)

16. Remove the trunk side upper trim.(See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION [WGN].)

17. Disconnect the rear drain hose from the sunroof frame.

18. Remove the rear drain hose from the clips.

19. Pull the rear drain hose into the room side.

20. Remove the rear drain hose.