#
ON-BOARD DIAGNOSTIC TEST [L3 Turbo]

id0102b7801000

## DTCs Reading Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located at the left side of the center console.

3. Retrieve DTCs using the WDS or equivalent.

## Pending Trouble Code Access Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located on the left side of the center console.

3. Retrieve PENDING trouble codes using the WDS or equivalent.

## Freeze Frame PID Data Access Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located on the left side of the center console.

3. Record the FREEZE FRAME PID DATA using the WDS or equivalent.

## On-Board System Readiness Tests Access Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect WDS or equivalent to the vehicle DLC-2 16-pin connector located on the left side of the center console.

3. Monitor the OBD systems operating status using the WDS or equivalent.

## PID/DATA Monitor and Record Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located on the left side of the center console.

3. Access and monitor PIDs using the WDS or equivalent.

## Diagnostic Monitoring Test Results Access Procedure

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located on the left side of the center console.

3. Access to the DIAGNOSTIC MONITORING TEST RESULTS and read the test results using the WDS or equivalent.