#
CONDENSER REMOVAL/INSTALLATION [4SD, 5HB]

id0920008030b6

## 4SD

1. Disconnect the negative battery cable.

2. Remove the rear package trim.

3. Remove in the order indicated in the table.

1 | Bolt
2 | Connector
3 | Condenser

4. Install in the reverse order of removal.

## 5HB

1. Disconnect the negative battery cable.

2. Remove the liftgate lower trim.

3. Remove in the order indicated in the table.

1 | Bolt
2 | Connector
3 | Condenser

4. Install in the reverse order of removal.