#
KNOCK SENSOR (KS) REMOVAL/INSTALLATION [L3 Turbo]

id0140b6802900

  Caution

  • Be careful not to impact the sensor.
  • Verify that there is no debris between the sensor and the cylinder block before installing.

1. Remove the intake manifold. (SeeINTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo])

2. Remove the KS attachment bolt to remove the KS.

3. Install in the reverse order of removal.

Tightening torque

  16-24 N·m {1.7-2.4 kgf·m, 12-17 ft·lbf}