#
STEERING GEAR AND LINKAGE INSPECTION

id061400801100

## Rack Inspection

1. Inspect the rack for cracking, damage, and tooth wear. Replace it as necessary.

2. Measure the runout of the rack.

Steering rack runout

  Large diameter portion (near point A): 0.15 mm {0.006 in} max.
  Small diameter portion (near point B): 0.20 mm {0.008 in} max.

3. If not within the specification, replace the rack.

## Tie-rod End Inspection

1. Inspect the tie-rod end for damage and boot cracks. Replace it as necessary.

2. Inspect the ball joint for looseness. Replace the tie-rod end as necessary.

3. Rotate the ball joint five times.

4. Measure the rotation torque of the ball joint using the SST and a pull scale.

Tie-rod end rotational torque

  0.6-2.0 N·m {6.2-20.3 kgf·cm, 5.4-17.7 in·lbf}
  [Pull scale reading 6.0-20.0 N {0.62-2.03 kgf, 1.4-4.4 lbf}]

5. If not within the specification, replace the tie-rod end.

## Tie rod Inspection

1. Inspect the tie rod for bending and damage. Replace it as necessary.

2. Inspect the ball joint for looseness. Replace the tie rod as necessary.

3. Swing the tie rod five times.

4. Measure the swinging torque using a pull scale.

Tie rod swing torque

  0.4-4.0 N·m {4.1-40.7 kgf·cm, 3.6-35.4 in·lbf}
  [Pull scale reading 4.0-40.0 N {0.41-4.07 kgf, 0.9-8.9 lbf}]

5. If not within the specification, replace the tie-rod.