#
HVAC SYSTEM WIRING DIAGRAM

id070300800100

Full-auto air conditioner

.

1 | Ambient temperature sensor
2 | Cabin temperature sensor
3 | Evaporator temperature sensor
4 | Water temperature sensor
5 | Solar radiation sensor
6 | From TNS relay
7 | Panel light control
8 | Climate control unit
9 | Each switch
10 | Refrigerant pressure switch
11 | Airflow mode actuator
12 | Air mix actuator
13 | Air intake actuator
14 | From blower relay
15 | Blower motor
16 | Power MOS FET
17 | From rear window defroster relay

Manual air conditioner

.

1 | Blower relay
2 | Blower motor
3 | Resistor
4 | Climate control unit
5 | Defroster switch
6 | From PCM
7 | Refrigerant pressure switch
8 | Ambient temperature sensor
9 | Evaporator temperature sensor
10 | Air intake actuator
11 | Center panel
12 | A/C relay
13 | Magnetic clutch
14 | To PCM
15 | This terminal is defroster switch terminal