#
INPUT/TURBINE SPEED SENSOR INSPECTION [FS5A-EL]

id051721801200

  Caution

  • Water or foreign objects entering the connector can cause a poor connection or corrosion. Be sure not to drop water or foreign objects on the connector when disconnecting it.

1. Disconnect the negative battery cable.

2. Remove the battery and battery tray.

3. Remove the air cleaner component. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L8, LF, L3].)

4. Disconnect the input/turbine speed sensor connector.

5. Measure resistance between the terminals of the input/turbine speed sensor.

  • If not as specified, replace the input/turbine speed sensor.

Input/turbine speed sensor resistance

  250-600 ohms (ATF temperature: -40-160 °C {-40-320 °F})

6. Connect the input/turbine speed sensor connector.

7. Install the air cleaner component. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L8, LF, L3].)

8. Install the battery and battery tray.

9. Connect the negative battery cable.