#
ABS (ABS/TCS) HU/CM REMOVAL/INSTALLATION [ATX]

id0413008025a4

  Caution

  • When replacing the ABS (ABS/TCS) HU/CM, the configuration procedure must be done before removing the ABS (ABS/TCS) HU/CM. If the configuration is not completed before removing the ABS (ABS/TCS) HU/CM, ABS (ABS/TCS) will not work properly after installation of the ABS (ABS/TCS) HU/CM.
  • Do not drop the ABS (ABS/TCS) HU/CM. Replace it if it is subjected to an impact.

1. Configurate the ABS (ABS/TCS) HU/CM (only when replacing it). (See ABS (ABS/TCS) HU/CM CONFIGURATION.)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Connector (See Connector Removal Note) (See Connector Installation Note
2 | Brake pipe (See Brake Pipe Removal Note) (See Brake Pipe Installation Note)
3 | Nut
4 | ABS (ABS/TCS) HU/CM (See ABS (ABS/TCS) HU/CM Removal/Installation Note)
5 | Stud

## Connector Removal Note

1. Release the lock lever to unlock it.

2. Remove the connector.

## Brake Pipe Removal Note

1. Mark the brake pipe connecting positions before removal for reference during installation.

## ABS (ABS/TCS) HU/CM Removal/Installation Note

1. When removing/installing the ABS (ABS/TCS) HU/CM from/to the vehicle, attach a strip of protective tape on the ABS (ABS/TCS) HU/CM connector to prevent brake fluid from entering.

## Brake Pipe Installation Note

1. When installing the brake pipe, align the marks made before removal with the ABS (ABS/TCS) HU/CM as shown in the figure.

## Connector Installation Note

1. Verify that the lock lever of the harness connector is securely locked.