#
DTC TABLE [BCM]

id0902j0837000

DTC No. | Description | Detection condition | Page
--- | --- | --- | ---
B1317 | Battery voltage high | Input voltage from the battery is excessively high | (See DTC B1317.)
B1318 | Battery voltage low | Input voltage from the battery is excessively low | (See DTC B1318.)
B1342 | ECU is faulted | BCM microcomputer malfunction | (See DTC B1342.)
B2572 | Driver door lock switch short to ground | Short to GND in wiring harness between BCM and driver-side door lock-link switch | (See DTC B2572.)
B2721 | Trunk lid ajar output short to ground | Short to GND in wiring harness between BCM and trunk compartment light switch | (See DTC B2721.)
B1873 | Turn signal/hazard power feed circuit short to ground | Short to GND in wiring harness between BCM and hazard warning switch | (See DTC B1873.)
B1320 | Door ajar LF circuit open | Open circuit in wiring harness between BCM and door switch (driver-side) | (See DTC B1320.)
B1328 | Door ajar RF circuit open | Open circuit in wiring harness between BCM and door switch (passenger-side) | (See DTC B1328.)
B1572 | Door ajar LR circuit open | Open circuit in wiring harness between BCM and door switch (LH) | (See DTC B1572.)
B1614 | Rear wiper interval switch input circuit short to ground | Short to GND in wiring harness between BCM and rear wiper and washer switch (INT) | (See DTC B1614.)
B2177 | Intruder sensor circuit failure | Short to GND in wiring harness between BCM and intruder sensor | (See DTC B2177.)
B1520 | Bonnet latch switch circuit open | Open circuit in wiring harness between BCM and bonnet latch switch | (See DTC B1520.)
B1506 | Light turn signal right circuit short to ground | Short to GND in wiring harness between BCM and turn switch | (See DTC B1506.)
B1311 | Unlock switch circuit open | Open circuit in wiring harness between BCM and driver-side door lock-link switch (unlock signal) | (See DTC B1311.)