#
DTC U0073, U2516

id0902e6901900

DTC | U0073 | PCM TCM ABS (ABS/TCS) HU/CM DSC HU/CM 4WD control module Keyless control module | CAN system communication error
--- | --- | --- | ---
U2516 | Instrument cluster
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection according to only detection conditions may cause injury due to operating error, or damage the system. When performing an inspection, always follow the inspection procedure. • CAN system related harness malfunction • Related module communication error
POSSIBLE CAUSE | • Open or short circuit in wiring harness • Malfunction of connectors between PCM, ABS (ABS/TCS) HU/CM, DSC HU/CM, TCM, 4WD control module, keyless control module and instrument cluster • PCM malfunction • TCM malfunction • ABS (ABS/TCS) HU/CM malfunction • DSC HU/CM malfunction 4WD control module malfunction • Keyless control module malfunction • Instrument cluster malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT CAN SYSTEM-RELATED DTC • Are any DTCs other than the following displayed? - U0073 - U2516 | Yes | Determine malfunctioning part in CAN system. (See PROCEDURES FOR DETERMINING THE LOCATION OF A MALFUNCTION)
No | Go to the next step.
2 | INSPECT CONNECTOR • Inspect the connector of the module that outputs the DTC. • Is it normal? | Yes | Go to the next step.
No | Repair or replace the connector, then go to Step 4.
3 | INSPECT WIRING HARNESSES • Inspect for the following malfunctioning wiring harnesses: - Short to GND - Short to power supply - Twisted pair short each other - Open circuit • Is there any malfunction? | Yes | Replace the wiring harness, then go to the next step.
No | Go to the next step.
4 | VERIFY TROUBLESHOOTING COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the module that outputs the DTC, then retry this step.
No | Troubleshooting completed.