REAR DRAIN HOSE INSTALLATION

id091500801600

  Caution
  • If the rear drain hose is pinched or bent anywhere, the water in the hose may not discharge and enter the inside of the vehicle. During and after installation of the trims and the headliner, always make sure there is no interference with the rear drain hose. Fix any problem if found.

1. Apply soapy water to the rear drain hose inserting area.

2. Insert one end (the wider side) of the rear drain hose into the sunroof frame.

3. Install the rear drain hose to the clips parallel to the pillar and free of slack.

4. Insert the rear drain hose joint into the rear pillar inner hole.

5. Install the following parts:

  (1) Headliner (See HEADLINER REMOVAL/INSTALLATION.)

  (2) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)

  (3) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)

  (4) Intruder sensor (vehicles with intruder sensor) (See INTRUDER SENSOR REMOVAL/INSTALLATION.)

  (5) Front map light (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

  (6) D-pillar trim (See D-PILLAR TRIM REMOVAL/INSTALLATION.)

  (7) Third-row seat belt upper anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (8) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)

  (9) Second-row seat belt upper anchor installation bolt (See SECOND-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (10) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (11) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (12) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (13) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (14) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (15) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (16) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (17) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

  (18) Front seat belt upper anchor installation bolt (Driver side) (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (19) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (20) Front seat belt lower anchor installation bolt. (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (21) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (22) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (23) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

6. Install the seaming welt.