WHEEL HUB COMPONENT REMOVAL/INSTALLATION [2WD]

id0312008004a1

  Caution
  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the wiring harness if it is pulled by mistake. Before performing the following procedures, disconnect the ABS wheel-speed sensor connector (body side) and fix the wiring harness to an appropriate place where it will not be pulled by mistake while servicing the vehicle.

1. Remove the rear ABS wheel-speed sensor. (See REAR ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION [2WD].)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

ac9wzw00000815

1 | Parking brake end cable (See PARKING BRAKE REMOVAL/INSTALLATION [2WD (L.H.D.)].) (See PARKING BRAKE REMOVAL/INSTALLATION [2WD (R.H.D.)].)
2 | Brake caliper component (See Brake Caliper Component Removal Note.)
3 | Disc plate (See REAR BRAKE (DISC) REMOVAL/INSTALLATION.)
4 | Wheel hub component
5 | Parking brake shoe component
6 | Wheel hub bolt (See Wheel Hub Bolt Removal Note.) (See Wheel Hub Bolt Installation Note.)

Brake Caliper Component Removal Note

1. Remove the brake caliper component from the trailing link and suspend it out of the way using a cable.

ac9uuw00001239

Wheel Hub Bolt Removal Note

  Note
  • The wheel hub bolts do not need to be removed unless they are being replaced.

1. Remove the wheel hub bolt using a press.

ac9uuw00001240

Wheel Hub Bolt Installation Note

1. Install the new wheel hub bolt using a press.

ac9uuw00001241